Street audit form

|  |  |  |  |
| --- | --- | --- | --- |
| **Element** | **Evaluation criteria** | **Y/N** | **Comments** |
| Footpath | Height of at least 150 mm and no more than 200 mm. |  |  |
| Minimum 2 m clear width in all locations. |  |  |
| Wheelchair kerb ramps have a maximum slope of 1:12. |  |  |
| Bollards installed along the edge of the footpath to prevent driving and parking on the footpath. |  |  |
| At least one set of bollards with spacing of 1,200 mm. |  |  |
| The footpath surface is uniform and non-slippery, with slope of 1:100 to avoid water stagnation. |  |  |
| Tactile warning are strips located at transition points (e.g., midblock crossings, intersections). |  |  |
| Cycle track | Physically separated cycle track with ≥ 2 m clear width. |  |  |
| Property entrances | The footpath remains at the same level through property entrances. |  |  |
| Bollards are installed on either side of each entrance to prevent driving and parking. |  |  |
| Property access is provided at a discrete location for each plot, with a maximum entrance width of 6 m. |  |  |
| Midblock crossings | Pedestrian crossings at intervals of 100-150 m. |  |  |
| Crossing are raised to the level of the footpath with ramps for vehicles (minimum slope of 1:8) OR have kerb ramps at each end of the crossing. |  |  |
| Median refuge islands are provided at crossing points, with minimum dimensions of 2 m by 1 m. |  |  |
| Intersection | Kerb ramps on all corners of intersections to provide wheelchair access to the footpath. |  |  |
| Median refuge islands with minimum dimensions of 2 m by 1 m on all arms with more than 2 lanes to cross. |  |  |
| Signalisation if any arm has more than 2 lanes to cross. |  |  |
| Pedestrian crossings are located along desire lines. |  |  |
| Turning radii are no more than 5 m. |  |  |
| Shade | Tree pits least every 20 m. |  |  |
| Lighting | No dark spots on footpath or carriageway. |  |  |
| On-street parking | Parking is provided in parallel orientation rather than angled or perpendicular parking. |  |  |
| Car parking bay size is no more than 5.0 m x 2.0 m |  |  |
| Street vending | The design includes designated spaces for organized street vending. |  |  |